{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sklop 1","Sklop 2"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sklop 1","index":0,"n_rows":70,"n_cols":8,"rows_kept":70,"merged":[[2,1,13,1],[14,1,26,1],[27,1,43,1],[44,1,48,1],[49,1,59,1],[65,0,65,1],[65,6,65,7]],"flags":["formulas_cached_only"]}
[null,"PONUDBENI PREDRAČUN (OBR-6b) - NN in SN talilni vložki - Sklop 1"]
["Zap. št.","Opis blaga","Nazivni tok","Proizvajalec/tip","Količina","EM","Cena za EM brez DDV (€)","Vrednost brez DDV (€)"]
["1.","NN TALILNI VLOŽEK; Un= 400 V, tip NV 00 (NV/NH 100), gG (gL) s središčnim indikatorjem","10A",null,211,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["2.",null,"16 A",null,{"v":1876,"d":"1,876"},"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["3.",null,"20 A",null,{"v":15695,"d":"15,695"},"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["4.",null,"25 A",null,{"v":9087,"d":"9,087"},"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["5.",null,"35 A",null,{"v":5911,"d":"5,911"},"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["6.",null,"40 A",null,213,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["7.",null,"50 A",null,{"v":3072,"d":"3,072"},"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["8.",null,"63 A",null,{"v":2005,"d":"2,005"},"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["9.",null,"80 A",null,878,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["10.",null,"100 A",null,{"v":1306,"d":"1,306"},"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["11.",null,"125 A",null,163,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["12.",null,"160 A",null,117,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["13."," NN TALILNI VLOŽEK; Un= 400 V, tip NV 1 (NV/NH 250),  gG (gL), s središčnim indikatorjem","16 A",null,148,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["14.",null,"20 A",null,571,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["15.",null,"25 A",null,531,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["16.",null,"35 A",null,507,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["17.",null,"50 A",null,{"v":1374,"d":"1,374"},"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["18.",null,"63 A",null,{"v":1481,"d":"1,481"},"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["19.",null,"80 A",null,848,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["20.",null,"100 A",null,442,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["21.",null,"125 A",null,246,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["22.",null,"160 A",null,60,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["23.",null,"200 A",null,76,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["24.",null,"224 A",null,29,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["25.",null,"250 A",null,96,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["26.","NN TALILNI VLOŽEK; Un= 400 V, tip NV 2 (NV/NH 400),   gG (gL), s središčnim indikatorjem","20 A",null,16,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["27.",null,"25 A",null,64,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["28.",null,"35 A",null,264,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["29.",null,"50 A",null,923,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["30.",null,"63 A",null,996,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["31.",null,"80 A",null,{"v":1036,"d":"1,036"},"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["32.",null,"100 A",null,490,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["33.",null,"125 A",null,377,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["34.",null,"160 A",null,385,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["35.",null,"200 A",null,237,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["36.",null,"224 A",null,31,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["37.",null,"250 A",null,132,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["38.",null,"280 A",null,1,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["39.",null,"300 A",null,43,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["40.",null,"315 A",null,63,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["41.",null,"355 A",null,51,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["42.",null,"400 A",null,33,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["43.","NN TALILNI VLOŽEK; Un= 400 V, tip NV 3 (NV/NH 630),   gG (gL), s središčnim indikatorjem","300 A",null,1,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["44.",null,"400 A",null,11,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["45.",null,"425 A",null,1,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["46.",null,"450 A",null,15,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["47.",null,"630 A",null,18,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["48.","SN TALILNI VLOŽEK; Un=24 kV; sila udarne igle = 80 N","6A",null,74,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["49.",null,"10A",null,240,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["50.",null,"16 A",null,165,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["51.",null,"20 A",null,134,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["52.",null,"25 A",null,92,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["53.",null,"30 A",null,51,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["54.",null,"40 A",null,52,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["55.",null,"50 A",null,60,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["56.",null,"63 A",null,23,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["57.",null,"80 A",null,1,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["58.",null,"100 A",null,16,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
[null,"Skupna vrednost brez DDV v (€):",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"22% DDV v (€):",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"Skupna vrednost z DDV v (€):",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
["Kraj in datum:",{"$nulls":5},"Podpis odgovorne osebe:"]
[]
[]
[]
["Ponudnik mora v kolikor posluje z žigom, ponudbeni predračun žigosati!"]

{"sheet":"Sklop 2","index":1,"n_rows":27,"n_cols":8,"rows_kept":27,"merged":[[1,0,3,0],[1,1,3,1],[1,2,3,2],[1,3,3,3],[1,4,3,4],[1,5,3,5],[1,6,3,6],[1,7,3,7],[17,0,17,6],[18,0,18,6],[19,0,19,6]],"flags":["formulas_cached_only"]}
[null,"PONUDBENI PREDRAČUN (OBR-6b) - NV stikalne letve in varovalčni ločilniki - Sklop 2"]
["Zap. št.","Opis blaga / storitve","Proizvajalec","Oznaka/tip","Količina","EM","Cena za EM brez DDV (€)","Vrednost brez DDV (€)"]
[]
[]
["1.","Stikalna letev NV 00 (160)/100 vertikalna",null,null,243,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["2.","Stikalna letev NV 00 (160)/185 vertikalna",null,null,2339,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["3.","Stikalna letev NV 2 (400)/185 vertikalna",null,null,622,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["4.","Stikalna letev NV 3 (630)/185 vertikalna",null,null,43,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["5.","Varovalčni ločilnik 3-polni NV 000 (100)/horizontalni, odvod zgoraj",null,null,911,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["6.","Varovalčni ločilnik 3-polni NV 00 (160)/horizontalni",null,null,302,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["7.","Varovalčni ločilnik 3-polni NV 1 (250)/horizontalni",null,null,73,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["8.","Varovalčni ločilnik 3-polni NV 2 (400)/horizontalni",null,null,23,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["9.","Varovalčni ločilnik 3-polni NV 000 (100)-OZEK horizontalni, sistem 60 mm, odvod zgoraj",null,null,620,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["10.","Varovalčni ločilnik 3-polni NV 00 (160)/horizontalni, sistem 60 mm",null,null,723,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["11.","Varovalčni ločilnik 3-polni NV 1 (250)/horizontalni, sistem 60 mm",null,null,120,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["12.","Varovalčni ločilnik 3-polni NV 2 (400)/horizontalni, sistem 60 mm",null,null,4,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["13.","Nosilec 3-polni za zbiralke debeline 5x30 mm",null,null,470,"kos",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["          SKUPAJ BREZ DDV(€)",{"$nulls":6},{"v":0,"d":"0.00"}]
["          DDV(€)",{"$nulls":6},{"v":0,"d":"0.00"}]
["          SKUPAJ Z DDV(€)",{"$nulls":6},{"v":0,"d":"0.00"}]
[]
[]
["Kraj in datum:",{"$nulls":3},"Podpis odgovorne osebe"]
[]
[]
[]
["Ponudnik mora v kolikor posluje z žigom ponudbeni predračun tudi žigosati!"]